1.58. - 		
	Base
1.59. - 	
	Added Com In settings to Settings menu
1.62.1.2 -
	Fixed problem with crashing after downloading RP config
	Support COM port numbers above 9
1.62.1.4 - 
	Support tag6 transmitters by transformation to tag3.
1.62.1.5
	Do not send to clients broken messages (Serv>0)
1.62.1.6
	Fixed bug in last feature
1.62.1.7
	Fixed problem with COM place in list
1.62.1.8
	Now is possible to set the computer time to the output messages by means of following strings in 	RPT_Serv.ini:
	for messages from COM port:
		[ComIn]
		PcTime=1
	for messages by IP:
		[In]
		PcTime=1
	Both parameter groups ([ComIn] & [In]) already exist in RPT_Serv.ini, you need to add a parameters only. The 	value by default for this parameters is 0.
1.62.1.9
	1. Added column “Comments” in main window. Is possible to describe comments, as a function of HpId 	parameter, in file comments.ini, what must be placed in main directory. Syntax of this file is following:
		[c]
		xxxxxx=<Repeater description>
	where xxxxxx – is HpId (left zeros may be removed)
	For each repeater must be inserted separate string. Number of strings not limited.
	2. For this version is needed new library file: db330d5r.bpl
1.62.1.10
	1. Changed algorithm of time sinchronization with repeaters.
1.62.1.12
	1. fixed bug with 7777/COM line position.
	2. fixed bug with    tag 6 to 3 transformation (missing of Test bit)
1.62.1.13
	1. Added setting for on/off removing duplicate messages from output's queue 
1.62.1.14
	1. fixed bug with    tag 6 to 3 transformation (Test acception)
1.62.1.16
	1. Fixed bug with RP signals transfer.
	2. Own RP tests now transfers as a general event
1.62.1.17
	1. Added option to remove test bit in messages from RT4-5seV4 (tag=6). For activating add string
		ClrTst6=1
to group [In] in file RPT_Serv.ini. In this case test message comes as Event only.
1.62.1.18
	1. Now in to log (RPT_Serv_c) is writing IP-address of client, not RPT only.
1.62.1.19
	1. Fixed bug with choising RP for programming.