1.14.6f - 
	Base
2.0.1 - 	
	Support of multiple GPRS chanels and CU-GSM pults
	Chage the priciples of transfer messages from WSC to GPRS modules (competible with WSC v5)
2.0.5.3 - 
	Add Log control and SMS_TCP port settings into the Settings menu
	Switching on or off Caller ID support for output messages
	Support CU-Gate as separate device (type 42)
	Support communication with HIT VMS program.
2.0.5.5 -	
	Add Search Service and duplicate phone numbers control in Editor for type 4x devices (CU-GSM and CU-	Gate).
2.0.5.6a
	Doesn't answer to messages from module, if it did not authorized before
2.0.5.7a (not work)
	add delay betwin strings when upload config ([Options] adelay=xx)
2.0.6.4
	1. Fixed problem with adelay parameter, recomended value for    adelay=5
	2. Support programming RR255 device (type 43)
	3. Cursor marks all string now and do not jump to first string on refresh.
2.0.6.5
	Fixed some bugs.
2.0.6.6
	Fixed bug with uploding programming data via COM-port (device types 41 and 42).
2.0.6.7
	Returned IP address identification for each connection.
2.0.6.8
	1. CRITICAL UPDATE! Fixed bug with incorrect connection identification when module configuration data is uploading.
	2. Widened a field in window for choising the connection (module) for programming.
2.0.6.9
	Fixed bug with CPU resourses usage in some configuration settings
2.0.6.10
	Fixed bug with data upload to CU-GSM and CU-Gate (types 41 and 42).
2.0.6.14
	1. Brodcast command sending once to each Online ID now. I.e. if module must reconnect after command accepting, this process will not be neverending.
	2. Broadcasting may be activate for each GPRS slot of TLF_Server separately.
	3. Broadcasting commands and broadcast enabling may be configured in Settings menu of TLF_Server.
	4. Broadcasting mode of GPRS slot are indicates by red color.
	5. Now is possible to sort objects in main window by MV field (module version).
2.0.6.18
	1. Included AutoUpdate feature for automatic FW update in GSM/GPRS modules. Is useable for 32xx and 34xx modules's FW versions.
	2. New version of library is used (db330d5r.bpl).
2.0.6.20
	1. Fixed bug with Auto Update.
2.0.6.23
	1. Fixed bug with stop working from incorrect messages, if CU-GSM is connected via TCP/IP.
2.0.6.24
	1. Fixed bug with closing connection in TCP_Drv slot.
2.0.6.25
	1. Fixed problem with long hex uploading to CU-GSM.
2.0.6.28
	1. Supports online programming and log viewing of modules version 34.3x (with Access feature)
2.0.6.31
	1. Now is possible to activate Module Config and Update features from main window via context menu.
2.0.6.32
	1. Now is limitation of max number of modules for one session in AutoUpdate mode.
2.0.6.38
	1. Now is possible to save to file list of connections with parameters (CSQ, version etc.).
	2. Opened transfer of Heartbeat from COM_IN to COM_OUT.
2.1.0.1
	1. Support programming RT4-5GP/4 devices.
	2. Fixed bug with opening SMS port when CU-GSM connected via IP.
2.1.0.2
	1. Fixed bug with V51xx programming.
	2. Now is possible to change message for OnLine mode monitoring (FF by default). For this purposes parameter TFormat= must be placed to [Options] group in TLF_Serv.ini file. 
Examle for Contact ID format message:
	[Options]
	TFormat=M06,%4.4x,EEEPPZZZ
where:	EEE – event code
	PP – partition
	ZZZ – zone number
2.1.0.4
	1. Fixed bug (TCP Port=0)
2.1.0.6
	1. Stopped unwanted messages from COM-IN  (MV:, V:, etc)
2.1.0.7
	1. Fixed bug (error with CU-GSM ethernet connection)
2.2.0.5
	1. Supports of  SIA DC-09-2021.
	2. Supports SIA format from GSM transceivers. 
	3. Enable programming modules types 51 and 52.
2.3.0.4
	1. Fixed bugs
2.3.0.6
	1. Fixed problem with hanging out of buffer.
	2. Added programming function Replace Account 
2.3.0.7
	1. Remove heartbeat from TLF_Serv log
2.3.0.8
	1. Add checkbox “TLM anable” to Module Config for RT4-5GT/4 (V52xx)
2.3.0.9
	1. Fixed bug: setting LifeTime in SIA_IP tab didn’t works.
	2. Remove ping of SIA_IP devices from output stream.
2.3.0.10
	1. Replace 0000 account from COM also in Contact ID format.
2.3.0.11
	1. Supports of command sending from WinSC v.4.x.x
2.3.0.12
	1. Supports SIA format messages reception from CU-GSM. To CU-GSM must be sent command <*#0*:CE-> from TLF_Serv. IpClient.dll must be updated to version Ip_Client_0_26xx_51a.
	2. Fixed bug with some SIA messages reception.